IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [ContentGUID: , VersionGUID: 4abfd342-48fc-4804-aec7-e942e1565457, NumberOfSaves: 0]"
File name: "M_Vacuum Degasser_MEPcontent_TTM_C6100_NoXygen C6100_INT-EN.ifc"
Time stamp: "2025-07-09T13:31:31+02:00"
Preprocessor: "ODA SDAI 22.12"
Originating system: "Autodesk Revit 23.1.60.36 (ENU) - IFC 23.4.0.0"
Application: "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)"

People and organizations
  Person "liviu_culica" of Organization (no name given)
  Owner history of Person "liviu_culica" of Organization (no name given) | application "Autodesk Revit 2023 (ENU)" version "2023" identifier "Revit" by Organization "Autodesk Revit 2023 (ENU)" | change NOCHANGE | created 1752057091 (2025-07-09T10:31:31Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  POWERUNIT: WATT
  VOLUMETRICFLOWRATEUNIT: derived
  FREQUENCYUNIT: HERTZ
  ELECTRICVOLTAGEUNIT: VOLT
  MASSUNIT: KILO GRAM

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "M_Vacuum Degasser_MEPcontent_TTM_C6100_INT-EN:NoXygen C6100" | object type "M_Vacuum Degasser_MEPcontent_TTM_C6100_INT-EN:NoXygen C6100" | names: "M_Vacuum Degasser_MEPcontent_TTM_C6100_INT-EN:NoXygen C6100:6330" | material: constituents ("Color RGB 040-040-040": "Color RGB 040-040-040", "Color RGB 130-130-130": "Color RGB 130-130-130", "Color RAL 9003": "Color RAL 9003", "Color RGB 130-141-149": "Color RGB 130-141-149", "Color RGB 255-015-015": "Color RGB 255-015-015") | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators, Other, Constraints, Dimensions, Electrical - Loads

Types
  IFCBUILDINGELEMENTPROXYTYPE "M_Vacuum Degasser_MEPcontent_TTM_C6100_INT-EN:NoXygen C6100" | 1 occurrence | material: constituents ("Equipment": "Color RGB 040-040-040", "Equipment": "Color RGB 130-130-130", "Equipment": "Color RAL 9003", "Equipment": "Color RGB 130-141-149", "Equipment": "Color RGB 255-015-015") | property sets: Other, Constraints, Dimensions, Electrical Engineering, Electrical - Loads, Identity Data

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "NoXygen C6100" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "NoXygen C6100" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Level 1" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level 1" (IFCLABEL)
    Type Id = "1899" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "M_Vacuum Degasser_MEPcontent_TTM_C6100_INT-EN" (IFCLABEL)
    Family and Type = "M_Vacuum Degasser_MEPcontent_TTM_C6100_INT-EN: NoXygen C6100" (IFCLABEL)
    Type = "NoXygen C6100" (IFCLABEL)
    Type Id = "6315" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Connection Diameter = 12.699999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Family Name = "M_Vacuum Degasser_MEPcontent_TTM_C6100_INT-EN" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "None" (IFCTEXT)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.016146778231853169 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00010326388256326011 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 type object
    Depth = 350. (IFCLENGTHMEASURE) [MILLI METRE]
    Diameter = 12.699999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1150. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Article Description = "Vacuum degasser for removal of dissolved gasses in heating and comfort cooling systems" (IFCTEXT)
    Article Type = "NoXygen C6100" (IFCTEXT)
    Base Family Version = "25.07" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Vacuum degasser for removal of dissolved gasses in heating and comfort cooling systems" (IFCTEXT)
    EMCS Version = "5.0" (IFCTEXT)
    ETIM Article Class = "EC002703" (IFCTEXT)
    Family Version = "25.07" (IFCTEXT)
    GTIN = "7331521519461" (IFCTEXT)
    MEPcontent Class = "VACUUM_DEGASSER" (IFCTEXT)
    Manufacturer = "TTM" (IFCTEXT)
    Manufacturer Art. No. = "519461" (IFCTEXT)
    Manufacturer URL = "https://ttmenergi.com/fluid-treatment/noxygen-degasser/ttm-noxygen-c6100/" (IFCTEXT)
    Model = "NoXygen C6100" (IFCTEXT)
    OmniClass Number = "23.75.50.11.14.14" (IFCTEXT)
    OmniClass Title = "Deaerators" (IFCTEXT)
    Product Line = "TTM" (IFCTEXT)
    Revit Version = "2023" (IFCTEXT)
    Type Name = "NoXygen C6100" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 type object
    Voltage = 400. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Power,Hydronic Return,Hydronic Supply" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Ambient Temperature = "0 – +40°C" (IFCTEXT)
    Classification = "None" (IFCIDENTIFIER)
    Media Temperature = "0 – 70°C" (IFCTEXT)
    Minimum Capacity, Degassed Liquid = 0.13500000000000004 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Noise Level = "61" (IFCTEXT)
    Pressure Stage = 13 (IFCINTEGER)
    Protection Class = "IP44" (IFCTEXT)
    Weight = 60. (IFCMASSMEASURE) [KILO GRAM]
  Mechanical - Flow | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Hydronic Return Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Electrical Engineering | properties | on 1 type object
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 3 (IFCINTEGER)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 040-040-040" (IFCLABEL)
    Grey = "Color RGB 130-130-130" (IFCLABEL)
    Light Blue = "Color RGB 130-141-149" (IFCLABEL)
    Red = "Color RGB 255-015-015" (IFCLABEL)
    White = "Color RAL 9003" (IFCLABEL)
    Yellow = "Color RGB 130-130-130" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "TTM" (IFCLABEL)